mididefault
Prev | Orchestra Opcodes and Operators | Next

## mididefault

mididefault — Changes values, depending on MIDI activation.

## Description

mididefault is designed to simplify writing instruments that can be used interchangeably for either score or MIDI input, and to make it easier to adapt instruments originally written for score input to work with MIDI input.

In general, it should be possible to write instrument definitions that work identically with both scores and MIDI, including both MIDI files and real-time MIDI input, without using any conditional statements, and that take full advantage of MIDI voice messages.

Note that correlating Csound instruments with MIDI channel numbers is done using the massign opcode for real-time performance,. For file-driven performance, instrument numbers default to MIDI channel number + 1, but the defaults are overridden by any MIDI program change messages in the file.

## Syntax

    mididefault xdefault, xvalue

## Performance

xdefault -- specifies a default value that will be used during MIDI activation.

xvalue -- overwritten by xdefault during MIDI activation, remains unchanged otherwise.

If the instrument was activated by MIDI input, the opcode will overwrite the value of xvalue with the value of xdefault. If the instrument was NOT activated by MIDI input, xvalue will remain unchanged.

This enables score pfields to receive a default value during MIDI activation, and score values otherwise.

| Adapting a score-activated Csound instrument.
- To adapt an ordinary Csound instrument designed for score activation for score/MIDI interoperability: Change all linen, linseg, and expseg opcodes to linenr, linsegr, and expsegr, respectively, except for a de-clicking or damping envelope. This will not materially change score-driven performance. Add the following lines at the beginning of the instrument definition:
      ; Ensures that a MIDI-activated instrument
      ; will have a positive p3 field.
      mididefault 60, p3
      ; Puts MIDI key translated to cycles per
      ; second into p4, and MIDI velocity into p5
      midinoteoncps p4, p5
Obviously, midinoteoncps could be changed to midinoteonoct or any of the other options, and the choice of p-fields is arbitrary.

## See Also

midichannelaftertouch, midicontrolchange, midinoteoff, midinoteoncps, midinoteonkey, midinoteonoct, midinoteonpch, midipitchbend, midipolyaftertouch, midiprogramchange

## Credits

Author: Michael Gogins

New in version 4.20

Prev | Up | Next
midictrl | Home | midiin