outipc
Prev | Orchestra Opcodes and Operators | Next

## outipc

outipc — Sends MIDI program change messages at i-rate

## Description

Sends MIDI program change messages at i-rate

## Syntax

    outipc ichn, iprog, imin, imax

## Initialization

ichn -- MIDI channel number (1-16)

iprog -- program change number in floating point

imin -- minimum floating point value (converted in MIDI integer value 0)

imax -- maximum floating point value (converted in MIDI integer value 127 (7 bit))

## Performance

outipc (i-rate program change output) sends program change messages. It works only with MIDI instruments which recognize them. It can drive a different value of a parameter for each note currently active.

It can scale an i-value floating-point argument according to the imin and imax values. For example, set imin = 1.0 and imax = 2.0. When the ivalue argument receives a 2.0 value, the opcode will send a 127 value to the MIDI OUT device. When the ivalue argument receives a 1.0 value, it will send a 0 value. i-rate opcodes send their message once during instrument initialization.

## See Also

outiat, outic14, outic, outipat, outipb, outkat, outkc14, outkc, outkpat, outkpb, outkpc

## Credits

Author: Gabriel Maldonado
Italy

New in Csound version 3.47

Thanks goes to Rasmus Ekman for pointing out the correct MIDI channel and controller number ranges.

Prev | Up | Next
outipb | Home | outkat