vco2ift
Prev | Orchestra Opcodes and Operators | Next

## vco2ift

vco2ift — Returns a table number at i-time for a given oscillator frequency and wavform.

## Description

vco2ift is the same as vco2ft, but works at i-time. It is suitable for use with opcodes that expect an i-rate table number (for example, oscili).

## Syntax

    ifn vco2ift icps, iwave [, inyx]

## Initialization

ifn -- the ftable number.

icps -- frequency in Hz. Zero and negative values are allowed. However, if the absolute value exceeds sr/2 (or sr*inyx), the selected table will contain silence.

iwave -- the waveform for which table number is to be selected. Allowed values are:

- 0: sawtooth

- 1: 4 * x * (1 - x) (integrated sawtooth)

- 2: pulse (not normalized)

- 3: square wave

- 4: triangle

Additionally, negative iwave values select user defined waveforms (see also vco2init).

inyx (optional, default=0.5) -- bandwidth of the generated waveform, as percentage (0 to 1) of the sample rate. The expected range is 0 to 0.5 (i.e. up to sr/2), other values are limited to the allowed range.

Setting inyx to 0.25 (sr/4), or 0.3333 (sr/3) can produce a “fatter” sound in some cases, although it is more likely to reduce quality.

## See Also

vco2ft, vco2init, and vco2.

## Credits

Author: Istvan Varga

New in version 4.22

Prev | Up | Next
vco2ft | Home | vco2init