atonek
Prev | Orchestra Opcodes and Operators | Next

## atonek

atonek — A notch filter whose transfer functions are the complements of the tone opcode.

## Description

A notch filter whose transfer functions are the complements of the tone opcode.

## Syntax

    kres atonek ksig, khp [, iskip]

## Initialization

iskip (optional, default=0) -- initial disposition of internal data space. Since filtering incorporates a feedback loop of previous output, the initial status of the storage space used is significant. A zero value will clear the space; a non-zero value will allow previous information to remain. The default value is 0.

## Performance

kres -- the output signal at control-rate.

ksig -- the input signal at control-rate.

khp -- the response curve's half-power point, in Hertz. Half power is defined as peak power / root 2.

atonek is a filter whose transfer functions is the complement of tonek. atonek is thus a form of high-pass filter whose transfer functions represent the “filtered out” aspects of their complements. However, power scaling is not normalized in atonek but remains the true complement of the corresponding unit.

## See Also

areson, aresonk, atone, port, portk, reson, resonk, tone, tonek

Prev | Up | Next
atone | Home | atonex