mpulse
Prev | Orchestra Opcodes and Operators | Next

## mpulse

mpulse — Generates a set of impulses.

## Description

Generates a set of impulses of amplitude kamp at frequency kfreq. The first impulse is after a delay of ioffset seconds. The value of kfreq is read only after an impulse, so it is the interval to the next impulse at the time of an impulse.

## Syntax

    ares mpulse kamp, kfreq [, ioffset]

## Initialization

ioffset (optional, default=0) -- the delay before the first impulse. If it is negative, the value is taken as the number of samples, otherwise it is in seconds. Default is zero.

## Performance

kamp -- amplitude of the impulses generated

kfreq -- frequency of the impulse train

After the initial delay, an impulse of kamp amplitude is generated as a single sample. Immediately after generating the impulse, the time of the next one is calculated. If kfreq is zero, there is an infinite wait to the next impulse. If kfreq is negative, the frequency is counted in samples rather than seconds.

## Examples

Here is an example of the mpulse opcode. It uses the files mpulse.orc and mpulse.sco.

Example 233. Example of the mpulse opcode.

    /* mpulse.orc */
    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1.
    instr 1
      ; Generate an impulse every 1/10th of a second.
      kamp = 30000
      kfreq = 0.1

      a1 mpulse kamp, kfreq
      out a1
    endin
    /* mpulse.orc */

    /* mpulse.sco */
    ; Play Instrument #1 for one second.
    i 1 0 1
    e
    /* mpulse.sco */

## Credits

Example written by Kevin Conder.

Prev | Up | Next
moscil | Home | mrtmsg