balance
Prev | Orchestra Opcodes and Operators | Next

## balance

balance — Adjust one audio signal according to the values of another.

## Description

The rms power of asig can be interrogated, set, or adjusted to match that of a comparator signal.

## Syntax

    ares balance asig, acomp [, ihp] [, iskip]

## Initialization

ihp (optional) -- half-power point (in Hz) of a special internal low-pass filter. The default value is 10.

iskip (optional, default=0) -- initial disposition of internal data space (see reson). The default value is 0.

## Performance

asig -- input audio signal

acomp -- the comparator signal

balance outputs a version of asig, amplitude-modified so that its rms power is equal to that of a comparator signal acomp. Thus a signal that has suffered loss of power (eg., in passing through a filter bank) can be restored by matching it with, for instance, its own source. It should be noted that gain and balance provide amplitude modification only - output signals are not altered in any other respect.

## Examples

Here is an example of the balance opcode. It uses the files balance.orc and balance.sco.

Example 37. Example of the balance opcode.

    /* balance.orc */
    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1.
    instr 1
      ; Generate a band-limited pulse train.
      asrc buzz 30000, 440, sr/440, 1

      ; Send the source signal through 2 filters.
      a1 reson asrc, 1000, 100
      a2 reson a1, 3000, 500

      ; Balance the filtered signal with the source.
      afin balance a2, asrc

      out afin
    endin
    /* balance.orc */

    /* balance.sco */
    ; Table #1, a sine wave.
    f 1 0 16384 10 1

    ; Play Instrument #1 for two seconds.
    i 1 0 2
    e
    /* balance.sco */

## See Also

gain, rms

Prev | Up | Next
babo | Home | bamboo