vcomb
Prev | Orchestra Opcodes and Operators | Next

## vcomb

vcomb — Variably reverberates an input signal with a “colored” frequency response.

## Description

Variably reverberates an input signal with a “colored” frequency response.

## Syntax

    ares vcomb asig, krvt, xlpt, imaxlpt [, iskip] [, insmps]

## Initialization

imaxlpt -- maximum loop time for klpt

iskip (optional, default=0) -- initial disposition of delay-loop data space (cf. reson). The default value is 0.

insmps (optional, default=0) -- delay amount, as a number of samples.

## Performance

krvt -- the reverberation time (defined as the time in seconds for a signal to decay to 1/1000, or 60dB down from its original amplitude).

xlpt -- variable loop time in seconds, same as ilpt in comb. Loop time can be as large as imaxlpt.

This filter reiterates input with an echo density determined by loop time ilpt. The attenuation rate is independent and is determined by krvt, the reverberation time (defined as the time in seconds for a signal to decay to 1/1000, or 60dB down from its original amplitude). Output will appear only after ilpt seconds.

## See Also

alpass, comb, reverb, valpass

## Credits

Author: William “Pete” Moss
University of Texas at Austin
Austin, Texas USA
January 2002

Prev | Up | Next
vco2init | Home | vcopy