oscil
Prev | Orchestra Opcodes and Operators | Next

## oscil

oscil — A simple oscillator.

## Description

Table ifn is incrementally sampled modulo the table length and the value obtained is multiplied by amp.

## Syntax

    ares oscil xamp, xcps, ifn [, iphs]

    kres oscil kamp, kcps, ifn [, iphs]

## Initialization

ifn -- function table number. Requires a wrap-around guard point.

iphs (optional, default=0) -- initial phase of sampling, expressed as a fraction of a cycle (0 to 1). A negative value will cause phase initialization to be skipped. The default value is 0.

## Performance

kamp, xamp -- amplitude

kcps, xcps -- frequency in cycles per second.

The oscil opcode generates periodic control (or audio) signals consisting of the value of kamp(xamp)times the value returned from control rate (audio rate) sampling of a stored function table. The internal phase is simultaneously advanced in accordance with the kcps or xcps input value.

## Examples

Here is an example of the oscil opcode. It uses the files oscil.orc and oscil.sco.

Example 248. Example of the oscil opcode.

    /* oscil.orc */
    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1 - a basic oscillator.
    instr 1
      kamp = 10000
      kcps = 440
      ifn = 1

      a1 oscil kamp, kcps, ifn
      out a1
    endin
    /* oscil.orc */

    /* oscil.sco */
    ; Table #1, a sine wave.
    f 1 0 16384 10 1

    ; Play Instrument #1 for 2 seconds.
    i 1 0 2
    e
    /* oscil.sco */

## See Also

oscili, oscil3

## Credits

Example written by Kevin Conder.

Prev | Up | Next
oscbnk | Home | oscil1