in32
Prev | Orchestra Opcodes and Operators | Next

## in32

in32 — Reads a 32-channel audio signal from an external device or stream.

## Description

Reads a 32-channel audio signal from an external device or stream.

## Syntax

    ar1, ar2, ar3, ar4, ar5, ar6, ar7, ar8, ar9, ar10, ar11, ar12, ar13, ar14, ar15, ar16, ar17, ar18, ar19, ar20, ar21, ar22, ar23, ar24, ar25, ar26, ar27, ar28, ar29, ar30, ar31, ar32 in32

## Performance

in32 reads a 32-channel audio signal from an external device or stream. If the command-line -i flag is set, sound is read continuously from the audio input stream (e.g. stdin or a soundfile) into an internal buffer.

## Credits

inch, inx, inz

## Credits

Author: John ffitch
University of Bath/Codemist Ltd.
Bath, UK
May 2000

New in Csound Version 4.07

Prev | Up | Next
in | Home | inch