pvsblur
Prev | Orchestra Opcodes and Operators | Next

## pvsblur

pvsblur — Average the amp/freq time functions of each analysis channel for a specified time.

## Description

Average the amp/freq time functions of each analysis channel for a specified time (truncated to number of frames). As a side-effect the input pvoc stream will be delayed by that amount.

## Syntax

    fsig pvsblur fsigin, kblurtime, imaxdel

## Performance

fsig -- output pv stream

fsigin -- input pv stream.

kblurtime -- time in secs during which windows will be averaged .

imaxdel -- maximum delay time, used for allocating memory used in the averaging operation.

This opcode will blur a pvstream by smoothing the amplitude and frequency time functions (a type of low-pass filtering); the amount of blur will depend on the length of the averaging period, larger blurtimes will result in a more pronounced effect.

## Examples

Example 299. Example

    asig  in                                 ; get the signal in

    fsig  pvsanal   asig, 1024, 256, 1024, 1 ; analyse it
    ftps  pvsblur   fsig, 0.2, 0.2           ; blur it for 200 ms
    atps  pvsynth   ftps                     ; synthesise it

## Credits

Author: Victor Lazzarini;
November 2004

New plugin in version 5

November 2004.

Prev | Up | Next
pvsfilter | Home | pvstencil