linenr
Prev | Orchestra Opcodes and Operators | Next

## linenr

linenr — The linen opcode extended with a final release segment.

## Description

linenr -- same as linen except that the final segment is entered only on sensing a MIDI note release. The note is then extended by the decay time.

## Syntax

    ares linenr xamp, irise, idec, iatdec

    kres linenr kamp, irise, idec, iatdec

## Initialization

irise -- rise time in seconds. A zero or negative value signifies no rise modification.

idur -- overall duration in seconds. A zero or negative value will cause initialization to be skipped.

idec -- decay time in seconds. Zero means no decay. An idec > idur will cause a truncated decay.

iatdec -- attenuation factor by which the closing steady state value is reduced exponentially over the decay period. This value must be positive and is normally of the order of .01. A large or excessively small value is apt to produce a cutoff which is audible. A zero or negative value is illegal.

## Performance

kamp, xamp -- input amplitude signal.

linenr is unique within Csound in containing a note-off sensor and release time extender. When it senses either a score event termination or a MIDI noteoff, it will immediately extend the performance time of the current instrument by idec seconds, then execute an exponential decay towards the factor iatdec. For two or more units in an instrument, extension is by the greatest idec.

linenr is an example of the special Csound “r” units that contain a note-off sensor and release time extender. When each senses a score event termination or a MIDI noteoff, it will immediately extend the performance time of the current instrument by idec seconds unless made independent by irind. Then it will begin a decay from wherever it was at the time.

These “r” units can also be modified by MIDI noteoff velocities (see veloffs). If the irind flag is on (non-zero), the overall performance time is unaffected by note-off and veloff data.

Multiple “r” units. When two or more “r” units occur in the same instrument it is usual to have only one of them influence the overall note duration. This is normally the master amplitude unit. Other units controlling, say, filter motion can still be sensitive to note-off commands while not affecting the duration by making them independent (irind non-zero). Depending on their own idec (release time) values, independent “r” units may or may not reach their final destinations before the instrument terminates. If they do, they will simply hold their target values until termination. If two or more “r” units are simultaneously master, note extension is by the greatest idec.

## See Also

envlpx, envlpxr, linen

Prev | Up | Next
linen | Home | lineto