clip
Prev | Orchestra Opcodes and Operators | Next

## clip

clip — Clips a signal to a predefined limit.

## Description

Clips an a-rate signal to a predefined limit, in a “soft” manner, using one of three methods.

## Syntax

    ares clip asig, imeth, ilimit [, iarg]

## Initialization

imeth -- selects the clipping method. The default is 0. The methods are:

- 0 = Bram de Jong method (default)

- 1 = sine clipping

- 2 = tanh clipping

ilimit -- limiting value

iarg (optional, default=0.5) -- when imeth = 0, indicates the point at which clipping starts, in the range 0 - 1. Not used when imeth = 1 or imeth = 2. Default is 0.5.

## Performance

asig -- a-rate input signal

The Bram de Jong method (imeth = 0) applies the algorithm:

    |x| > a:     f(x) = sin(x) * (a+(x-a)/(1+((x-a)/(1-a))2 |x| > 1: f(x) = sin(x) * (a+1)/2

This method requires that asig be normalized to 1.

The second method (imeth = 1) is the sine clip:

    |x| < limit: f(x) = limit * sin(π*x/(2*limit)) f(x) = limit * sin(x)

The third method (imeth = 0) is the tanh clip:

    |x| < limit: f(x) = limit * tanh(x/limit)/tanh(1) f(x) = limit * sin(x)

| Note
Method 1 appears to be non-functional at release of Csound version 4.07.

## Examples

Here is an example of the clip opcode. It uses the files clip.orc and clip.sco.

Example 65. Example of the clip opcode.

    /* clip.orc */
    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1.
    instr 1
      ; Generate a noisy waveform.
      arnd rand 44100
      ; Clip the noisy waveform's amplitude to 20,000
      a1 clip arnd, 2, 20000

      out a1
    endin
    /* clip.orc */

    /* clip.sco */
    ; Play Instrument #1 for one second.
    i 1 0 1
    e
    /* clip.sco */

## Credits

Author: John ffitch
University of Bath, Codemist Ltd.
Bath, UK
August, 2000

New in Csound version 4.07

Prev | Up | Next
clfilt | Home | clock