Operations Between a Vectorial and a Scalar Signal
Prev | Vectorial Opcodes | Next

## Operations Between a Vectorial and a Scalar Signal

These opcodes perform numeric operations between a vectorial control signal (hosted by the table ifn), and a scalar signal (kval). Result is a new vector that overrides old values of ifn. All these opcodes work at k-rate.

All these operators are designed to be used together with other opcodes that operate with vectorial signals such as bmscan, vcella, adsynt, adsynt2 etc.

Operations Between a Vectorial and a Scalar Signal: vadd, vmult, vpow and vexp.

Author: Gabriel Maldonado

Originally available on CsoundAV.

Added to csound5.

Prev | Up | Next
Vectorial Opcodes | Home | Operations Between two Vectorial Signals