delayr
Prev | Orchestra Opcodes and Operators | Next

## delayr

delayr — Reads from an automatically established digital delay line.

## Description

Reads from an automatically established digital delay line.

## Syntax

    ares delayr idlt [, iskip]

## Initialization

idlt -- requested delay time in seconds. This can be as large as available memory will permit. The space required for n seconds of delay is 4n * sr bytes. It is allocated at the time the instrument is first initialized, and returned to the pool at the end of a score section.

iskip (optional, default=0) -- initial disposition of delay-loop data space (see reson). The default value is 0.

## Performance

delayr reads from an automatically established digital delay line, in which the signal retrieved has been resident for idlt seconds. This unit must be paired with and precede an accompanying delayw unit. Any other Csound statements can intervene.

## Examples

See the example for delayw.

## See Also

delay, delay1, delayw

Prev | Up | Next
delayk | Home | delayw