aftouch
Prev | Orchestra Opcodes and Operators | Next

## aftouch

aftouch — Get the current after-touch value for this channel.

## Description

Get the current after-touch value for this channel.

## Syntax

    kaft aftouch [imin] [, imax]

## Initialization

imin (optional, default=0) -- minimum limit on values obtained.

imax (optional, default=127) -- maximum limit on values obtained.

## Performance

Get the current after-touch value for this channel. Note that this access to pitch-bend data is independent of the MIDI pitch, enabling the value here to be used for any arbitrary purpose.

## Examples

Here is an example of the aftouch opcode. It uses the files aftouch.orc and aftouch.sco.

Example 28. Example of the aftouch opcode.

    /* aftouch.orc */
    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1.
    instr 1
      k1 aftouch

      printk2 k1
    endin
    /* aftouch.orc */

    /* aftouch.sco */
    ; Play Instrument #1 for 12 seconds.
    i 1 0 12
    e
    /* aftouch.sco */

## See Also

ampmidi, cpsmidi, cpsmidib, midictrl, notnum, octmidi, octmidib, pchbend, pchmidi, pchmidib, veloc

## Credits

Author: Barry L. Vercoe - Mike Berry
MIT - Mills
May 1997

Example written by Kevin Conder.

Prev | Up | Next
aexprand | Home | agauss