rigoto
Prev | Orchestra Opcodes and Operators | Next

## rigoto

rigoto — Transfers control during a reinit pass.

## Description

Similar to igoto, but effective only during a reinit pass (i.e., no-op at standard i-time). This statement is useful for bypassing units that are not to be reinitialized.

## Syntax

    rigoto label

## See Also

cigoto, igoto, reinit, rireturn

Prev | Up | Next
rezzy | Home | rireturn