rireturn
Prev | Orchestra Opcodes and Operators | Next

## rireturn

rireturn — Terminates a reinit pass.

## Description

Terminates a reinit pass (i.e., no-op at standard i-time). This statement, or an endin, will cause normal performance to be resumed.

## Syntax

                rireturn

## Examples

The following statements will generate an exponential control signal whose value moves from 440 to 880 exactly ten times over the duration p3. They use the files reinit.orc and reinit.sco.

Example 327. Example of the rireturn opcode.

    /* reinit.orc */
    sr = 44100
    kr = 44100
    ksmps = 1
    nchnls = 1

    instr 1

    reset:
            timout 0, p3/10, contin
            reinit reset

    contin:
            kLine expon 440, p3/10, 880
            aSig oscil 10000, kLine, 1
            out aSig
            rireturn

    endin
    /* reinit.orc */

    /* reinit.sco */
    f1 0 4096 10 1

    i1 0 10
    e
    /* reinit.sco */

## See Also

reinit, rigoto

Prev | Up | Next
rigoto | Home | rms