oscil1
Prev | Orchestra Opcodes and Operators | Next

## oscil1

oscil1 — Accesses table values by incremental sampling.

## Description

Accesses table values by incremental sampling.

## Syntax

    kres oscil1 idel, kamp, idur, ifn

## Initialization

idel -- delay in seconds before oscil1 incremental sampling begins.

idur -- duration in seconds to sample through the oscil1 table just once. A zero or negative value will cause all initialization to be skipped.

ifn -- function table number. tablei, oscil1i require the extended guard point.

## Performance

kamp -- amplitude factor.

oscil1 accesses values by sampling once through the function table at a rate determined by idur. For the first idel seconds, the point of scan will reside at the first location of the table; it will then begin moving through the table at a constant rate, reaching the end in another idur seconds; from that time on (i.e. after idel + idur seconds) it will remain pointing at the last location. Each value obtained from sampling is then multiplied by an amplitude factor kamp before being written into the result.

## See Also

table, tablei, table3, oscil1i, osciln

Prev | Up | Next
oscil | Home | oscil1i