MixerReceive
Prev | Orchestra Opcodes and Operators | Next

## MixerReceive

MixerReceive — Receives an arate signal from a channel of a buss.

## Syntax

    asignal MixerReceive ibuss, ichannel

## Description

Receives an arate signal that has been mixed onto a channel of a buss.

## Initialization

ibuss -- The number of the buss, for example the number of the instrument receiving the signal.

ichannel -- The number of the channel. Each buss has `nchnls` channels.

## Performance

asignal -- The signal that has been mixed onto the indicated channel of the buss.

Use of the mixer requires that instruments setting gains have smaller numbers than instruments sending signals, and that instruments sending signals have smaller numbers than instruments receiving those signals. However, an instrument may have any number of sends or receives. After the final signal is received, MixerClear must be invoked to reset the busses to 0 before the next kperiod.

## Examples

    instr 220 ; Master output
        ; It applies a bass enhancement, compression and fadeout
        ; to the whole piece, outputs signals, and clears the mixer.
      a1  MixerReceive 220, 0
      a2  MixerReceive 220, 1
      ; Bass enhancement
      al1 butterlp a1, 100
      al2 butterlp a2, 100
      a1 = al1*1.5 +a1
      a2 = al2*1.5 +a2

      ; Global amplitude shape
      kenv   linseg 0., p5 / 2.0, p4, p3 - p5, p4, p5 / 2.0, 0.
      a1=a1*kenv
      a2=a2*kenv

      ; Compression
      a1 dam a1, 5000, 0.5, 1, 0.2, 0.1
      a2 dam a2, 5000, 0.5, 1, 0.2, 0.1

      ; Remove DC bias
      a1blocked 	dcblock		a1
      a2blocked	dcblock		a2

      ; Output signals
      outs a1blocked, a2blocked
      MixerClear
    endin

## Credits

Michael Gogins (gogins at pipeline dot com).

Prev | Up | Next
MixerSend | Home | MixerClear