chano
Prev | Orchestra Opcodes and Operators | Next

## chano

chano — Send data to the outwards software bus

## Description

Send data to a channel of the outward software bus.

## Syntax

     chano kval, kchan

     chano aval, kchan

## Initialization

## Performance

xval --- value to transmit

kchan -- a positive integer that indicates which channel of the software bus to write

Note that the inward and outward software busses are independent, and are not mixer buses. The last value remains until a new value is written. There is no imposed limit to the number of busses but they use memory so small numbers are to be preferred.

## Example

The example shows the software bus being used as an asynchronous control signal to select a filter cutoff. It assumes that an external program that has access to the API is feeding the values

            sr = 44100
            ksmps = 100
            nchnls = 1

            instr   1
               a1   oscil     p4, p5, 100
                    chano     1, a1
            endin

## Credits

Author: John ffitch
2005

Prev | Up | Next
chani | Home | checkbox