tbvcf
Prev | Orchestra Opcodes and Operators | Next

## tbvcf

tbvcf — Models some of the filter characteristics of a Roland TB303 voltage-controlled filter.

## Description

This opcode attempts to model some of the filter characteristics of a Roland TB303 voltage-controlled filter. Euler's method is used to approximate the system, rather than traditional filter methods. Cutoff frequency, Q, and distortion are all coupled. Empirical methods were used to try to unentwine, but frequency is only approximate as a result. Future fixes for some problems with this opcode may break existing orchestras relying on this version of tbvcf.

## Syntax

    ares tbvcf asig, xfco, xres, kdist,
        kasym [, iskip]

## Initialization

iskip (optional, default=0) -- if non zero skip the initialisation of the filter. (New in Csound version 4.23f13 and 5.0)

## Performance

asig -- input signal. Should be normalized to ±1.

xfco -- filter cutoff frequency. Optimum range is 10,000 to 1500. Values below 1000 may cause problems.

xres -- resonance or Q. Typically in the range 0 to 2.

kdist -- amount of distortion. Typical value is 2. Changing kdist significantly from 2 may cause odd interaction with xfco and xres.

kasym -- asymmetry of resonance. Typically in the range 0 to 1.

## Examples

Here is an example of the tbvcf opcode. It uses the files tbvcf.orc and tbvcf.sco.

Example 372. Example of the tbvcf opcode.

    /* tbvcf.orc */
    ;---------------------------------------------------------
    ; TBVCF Test
    ; Coded by Hans Mikelson December, 2000
    ;---------------------------------------------------------
      sr =  44100   ; Sample rate
      kr =  4410   ; Kontrol rate
      ksmps =  10   ; Samples/Kontrol period
      nchnls =  2        ; Normal stereo
      zakinit 50, 50

              instr 10

      idur    =          p3                                ; Duration
      iamp    =          p4                                ; Amplitude
      ifqc    =          cpspch(p5)                        ; Pitch to frequency
      ipanl   =          sqrt(p6)                          ; Pan left
      ipanr   =          sqrt(1-p6)                        ; Pan right
      iq      =          p7
      idist   =          p8
      iasym   =          p9

      kdclck  linseg 0, .002, 1, idur-.004, 1, .002, 0 ; Declick envelope

      kfco    expseg 10000, idur, 1000                 ; Frequency envelope

      ax      vco 1, ifqc, 2, 1                     ; Square wave
      ay      tbvcf ax, kfco, iq, idist, iasym        ; TB-VCF
      ay      buthp ay/1, 100                         ; Hi-pass

              outs ay*iamp*ipanl*kdclck, ay*iamp*ipanr*kdclck
              endin
    /* tbvcf.orc */

    /* tbvcf.sco */
    f1 0 65536 10 1

    ; TeeBee Test
    ;   Sta  Dur  Amp    Pitch Pan  Q    Dist1 Asym
    i10 0    0.2  32767  7.00  .5   0.0  2.0   0.0
    i10 0.3  0.2  32767  7.00  .5   0.8  2.0   0.0
    i10 0.6  0.2  32767  7.00  .5   1.6  2.0   0.0
    i10 0.9  0.2  32767  7.00  .5   2.4  2.0   0.0
    i10 1.2  0.2  32767  7.00  .5   3.2  2.0   0.0
    i10 1.5  0.2  32767  7.00  .5   4.0  2.0   0.0
    i10 1.8  0.2  32767  7.00  .5   0.0  2.0   0.25
    i10 2.1  0.2  32767  7.00  .5   0.8  2.0   0.25
    i10 2.4  0.2  32767  7.00  .5   1.6  2.0   0.25
    i10 2.7  0.2  32767  7.00  .5   2.4  2.0   0.25
    i10 3.0  0.2  32767  7.00  .5   3.2  2.0   0.25
    i10 3.3  0.2  32767  7.00  .5   4.0  2.0   0.25
    i10 3.6  0.2  32767  7.00  .5   0.0  2.0   0.5
    i10 3.9  0.2  32767  7.00  .5   0.8  2.0   0.5
    i10 4.2  0.2  32767  7.00  .5   1.6  2.0   0.5
    i10 4.5  0.2  32767  7.00  .5   2.4  2.0   0.5
    i10 4.8  0.2  32767  7.00  .5   3.2  2.0   0.5
    i10 5.1  0.2  32767  7.00  .5   4.0  2.0   0.5
    i10 5.4  0.2  32767  7.00  .5   0.0  2.0   0.75
    i10 5.7  0.2  32767  7.00  .5   0.8  2.0   0.75
    i10 6.0  0.2  32767  7.00  .5   1.6  2.0   0.75
    i10 6.3  0.2  32767  7.00  .5   2.4  2.0   0.75
    i10 6.6  0.2  32767  7.00  .5   3.2  2.0   0.75
    i10 6.9  0.2  32767  7.00  .5   4.0  2.0   0.75
    i10 7.2  0.2  32767  7.00  .5   0.0  2.0   1.0
    i10 7.5  0.2  32767  7.00  .5   0.8  2.0   1.0
    i10 7.8  0.2  32767  7.00  .5   1.6  2.0   1.0
    i10 8.1  0.2  32767  7.00  .5   2.4  2.0   1.0
    i10 8.4  0.2  32767  7.00  .5   3.2  2.0   1.0
    i10 8.7  0.2  32767  7.00  .5   4.0  2.0   1.0
    e
    /* tbvcf.sco */

## Credits

Author: Hans Mikelson
December, 2000 -- January, 2001

New in Csound 4.10

Prev | Up | Next
taninv2 | Home | tempest