adsr
Prev | Orchestra Opcodes and Operators | Next

## adsr

adsr — Calculates the classical ADSR envelope using linear segments.

## Description

Calculates the classical ADSR envelope using linear segments.

## Syntax

    ares adsr iatt, idec, islev, irel [, idel]

    kres adsr iatt, idec, islev, irel [, idel]

## Initialization

iatt -- duration of attack phase

idec -- duration of decay

islev -- level for sustain phase

irel -- duration of release phase

idel -- period of zero before the envelope starts

## Performance

The envelope is the range 0 to 1 and may need to be scaled further. The envelope may be described as:

Picture of an ADSR envelope.

The length of the sustain is calculated from the length of the note. This means adsr is not suitable for use with MIDI events. The opcode madsr uses the linsegr mechanism, and so can be used in MIDI applications.

adsr is new in Csound version 3.49.

## Examples

Here is an example of the adsr opcode. It uses the files adsr.orc and adsr.sco.

Example 25. Example of the adsr opcode.

    /* adsr.orc */
    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1 - a simple instrument.
    instr 1
      ; Set the amplitude.
      kamp init 20000
      ; Get the frequency from the fourth p-field.
      kcps = cpspch(p4)

      a1 vco kamp, kcps, 1
      out a1
    endin

    ; Instrument #2 - instrument with an ADSR envelope.
    instr 2
      iatt = 0.05
      idec =  0.5
      islev = 0.08
      irel = 0.008

      ; Create an amplitude envelope.
      kenv adsr iatt, idec, islev, irel
      kamp = kenv * 20000

      ; Get the frequency from the fourth p-field.
      kcps = cpspch(p4)

      a1 vco kamp, kcps, 1
      out a1
    endin
    /* adsr.orc */

    /* adsr.sco */
    ; Table #1, a sine wave.
    f 1 0 16384 10 1

    ; Set the tempo to 120 beats per minute.
    t 0 120

    ; Play a melody with Instrument #1.
    ; p4 = frequency in pitch-class notation.
    i  1  0   1  8.04
    i  1  1   1  8.04
    i  1  2   1  8.05
    i  1  3   1  8.07
    i  1  4   1  8.07
    i  1  5   1  8.05
    i  1  6   1  8.04
    i  1  7   1  8.02
    i  1  8   1  8.00
    i  1  9   1  8.00
    i  1  10  1  8.02
    i  1  11  1  8.04
    i  1  12  2  8.04
    i  1  14  2  8.02

    ; Repeat the melody with Instrument #2.
    ; p4 = frequency in pitch-class notation.
    i  2  16  1  8.04
    i  2  17  1  8.04
    i  2  18  1  8.05
    i  2  19  1  8.07
    i  2  20  1  8.07
    i  2  21  1  8.05
    i  2  22  1  8.04
    i  2  23  1  8.02
    i  2  24  1  8.00
    i  2  25  1  8.00
    i  2  26  1  8.02
    i  2  27  1  8.04
    i  2  28  2  8.04
    i  2  30  2  8.02
    e
    /* adsr.sco */

## See Also

madsr, mxadsr, xadsr

## Credits

Author: John ffitch

Example written by Kevin Conder.

Prev | Up | Next
active | Home | adsyn