Limiting and wrapping of vectorial control signals
Prev | Vectorial Opcodes | Next

## Limiting and wrapping of vectorial control signals

These opcodes are similar to limit, wrap and mirror, but operate with a vectorial signal instead of with a scalar signal.

Result overrides old values of ifn1, if these are out of min/max interval. If you want to keep input vector, use vcopy opcode to copy it in another table.

All these opcodes work at k-rate.

All these operators are designed to be used together with other opcodes that operate with vectorial signals such as bmscan, vcella, adsynt, adsynt2 etc.

Operations Between two Vectorial Signals: vlimit, vwrap and vmirror.

Author: Gabriel Maldonado

Originally available on CsoundAV.

Added to csound5.

Prev | Up | Next
Vectorial Envelope Generators | Home | Vectorial Control-rate Delay Paths