trsplit
Prev | Orchestra Opcodes and Operators | Next

## trsplit

trsplit — Streaming partial track frequency splitting.

## Description

The trsplit opcode takes an input containg a TRACKS pv streaming signal (as generated, for instance by partials) and splits it into two signals according to a k-rate frequency 'split point'. The first output will contain all tracks up from 0Hz to the split frequency and the second will contain the tracks from the split frequency up to the Nyquist. It can also, optionally, scale the gain of the output signals by a k-rate amount (default 1). The result is two output signals containing only part of the original spectrum.

## Syntax

    fsiglow, fsighi trsplit fin, ksplit[, kgainlow, kgainhigh]

## Performance

fsiglow -- output pv stream in TRACKS format containing the tracks below the split point.

fsighi -- output pv stream in TRACKS format containing the tracks above and including the split point.

fin -- input pv stream in TRACKS format

ksplit -- frequency split point in Hz

kgainlow, kgainhig -- amplitude scaling of each one of the outputs (default 1).

## Examples

Example 390. Example

    ain inch 1                  ; input signal
    fs1,fsi2 pvsifd ain,2048,512,1 ; ifd analysis
    fst  partials fs1,fsi2,.003,1,3,500  ; partial tracking
    fslo,fshi trsplit  fst, 1500 ; split partial tracks at 1500 Hz
          aout  tradsyn fshi, 1, 1, 500, 1 ; resynthesis of tracks above 1500Hz
    out aout

The example above shows partial tracking of an ifd-analysis signal and linear additive resynthesis of the upper part of the spectrum (from 1500Hz).

## Credits

Author: Victor Lazzarini;
February 2006

Prev | Up | Next
trshift | Home | turnoff