pvsvoc
Prev | Orchestra Opcodes and Operators | Next

## pvsvoc

pvsvoc — Combine the spectral envelope of one fsig with the excitation (frequencies) of another.

## Description

This opcode provides support for cross-synthesis of amplitudes and frequencies. It takes the amplitudes of one input fsig and combines with frequencies from another. It is a spectral version of the well-known channel vocoder.

## Syntax

    fsig pvsvoc famp, fexc, kdepth, kgain

## Performance

fsig -- output pv stream

famp -- input pv stream from which the amplitudes will be extracted

fexc -- input pv stream from which the frequencies will be taken

kdepth -- depth of effect, affecting how much of the frequencies will be taken from the second fsig: 0, the output is the famp signal, 1 the output is the famp amplitudes and fexc frequencies.

kgain -- gain boost/attenuation applied to the output.

## Examples

Example 301. Example

    asig  in                                 ; get the signal in
    asyn  oscili 16000, 150, 1               ; excitation signal

    famp  pvsanal   asig, 1024, 256, 1024, 1 ; analyse in signal
    fexc  pvsanal   asyn, 1024, 256, 1024, 1 ; analyse excitation signal
    ftps  pvsvoc   famp, fexc, 1, 1     ; cross it
    atps  pvsynth  ftps                      ; synthesise it

           out atps

The example above shows a typical cross-synthesis operation. The input signal (say a vocal sound) is used for its amplitude spectrum. An oscillator with an arbitrary complex waveform produces the excitation signal, giving the vocal sound its pitch.

## Credits

Author: Victor Lazzarini;
April 2005

New plugin in version 5

April 2005.

Prev | Up | Next
pvstencil | Home | pyassign Opcodes