midic21
Prev | Orchestra Opcodes and Operators | Next

## midic21

midic21 — Allows a floating-point 21-bit MIDI signal scaled with a minimum and a maximum range.

## Description

Allows a floating-point 21-bit MIDI signal scaled with a minimum and a maximum range.

## Syntax

    idest midic21 ictlno1, ictlno2, ictlno3, imin, imax [, ifn]

    kdest midic21 ictlno1, ictlno2, ictlno3, kmin, kmax [, ifn]

## Initialization

idest -- output signal

ictln1o -- most-significant byte controller number (0-127)

ictlno2 -- mid-significant byte controller number (0-127)

ictlno3 -- least-significant byte controller number (0-127)

imin -- user-defined minimum floating-point value of output

imax -- user-defined maximum floating-point value of output

ifn (optional) -- table to be read when indexing is required. Table must be normalized. Output is scaled according to the imin and imax values.

## Performance

kdest -- output signal

kmin -- user-defined minimum floating-point value of output

kmax -- user-defined maximum floating-point value of output

midic21 (i- and k-rate 21 bit MIDI control) allows a floating-point 21-bit MIDI signal scaled with a minimum and a maximum range. Minimum and maximum values can be varied at k-rate. It can use optional interpolated table indexing. It requires three MIDI controllers as input.

## See Also

ctrl7, ctrl14, ctrl21, initc7, initc14, initc21, midic7, midic14

## Credits

Author: Gabriel Maldonado
Italy

New in Csound version 3.47

Thanks goes to Rasmus Ekman for pointing out the correct MIDI channel and controller number ranges.

Prev | Up | Next
midic14 | Home | midic7