- NAME
- SYNOPSIS
- DESCRIPTION
- RETURN VALUES

# NAME

SSL_CTX_set_tlsext_status_cb, SSL_CTX_set_tlsext_status_arg, SSL_set_tlsext_status_type, SSL_get_tlsext_status_ocsp_resp, SSL_set_tlsext_status_ocsp_resp - OCSP Certificate Status Request functions

# SYNOPSIS

     #include <openssl/tls1.h>

     long SSL_CTX_set_tlsext_status_cb(SSL_CTX *ctx,
                                       int (*callback)(SSL *, void *));
     long SSL_CTX_set_tlsext_status_arg(SSL_CTX *ctx, void *arg);

     long SSL_set_tlsext_status_type(SSL *s, int type);

     long SSL_get_tlsext_status_ocsp_resp(ssl, unsigned char **resp);
     long SSL_set_tlsext_status_ocsp_resp(ssl, unsigned char *resp, int len);

# DESCRIPTION

A client application may request that a server send back an OCSP status response (also known as OCSP stapling). To do so the client should call the `SSL_set_tlsext_status_type()` function prior to the start of the handshake. Currently the only supported type is TLSEXT_STATUSTYPE_ocsp. This value should be passed in the type argument. The client should additionally provide a callback function to decide what to do with the returned OCSP response by calling SSL_CTX_set_tlsext_status_cb(). The callback function should determine whether the returned OCSP response is acceptable or not. The callback will be passed as an argument the value previously set via a call to SSL_CTX_set_tlsext_status_arg(). Note that the callback will not be called in the event of a handshake where session resumption occurs (because there are no Certificates exchanged in such a handshake).

The response returned by the server can be obtained via a call to SSL_get_tlsext_status_ocsp_resp(). The value *resp will be updated to point to the OCSP response data and the return value will be the length of that data. Typically a callback would obtain an OCSP_RESPONSE object from this data via a call to the `d2i_OCSP_RESPONSE()` function. If the server has not provided any response data then *resp will be NULL and the return value from `SSL_get_tlsext_status_ocsp_resp()` will be -1.

A server application must also call the `SSL_CTX_set_tlsext_status_cb()` function if it wants to be able to provide clients with OCSP Certificate Status responses. Typically the server callback would obtain the server certificate that is being sent back to the client via a call to SSL_get_certificate(); obtain the OCSP response to be sent back; and then set that response data by calling SSL_set_tlsext_status_ocsp_resp(). A pointer to the response data should be provided in the resp argument, and the length of that data should be in the len argument.

# RETURN VALUES

The callback when used on the client side should return a negative value on error; 0 if the response is not acceptable (in which case the handshake will fail) or a positive value if it is acceptable.

The callback when used on the server side should return with either SSL_TLSEXT_ERR_OK (meaning that the OCSP response that has been set should be returned), SSL_TLSEXT_ERR_NOACK (meaning that an OCSP response should not be returned) or SSL_TLSEXT_ERR_ALERT_FATAL (meaning that a fatal error has occurred).

SSL_CTX_set_tlsext_status_cb(), SSL_CTX_set_tlsext_status_arg(), `SSL_set_tlsext_status_type()` and `SSL_set_tlsext_status_ocsp_resp()` return 0 on error or 1 on success.

`SSL_get_tlsext_status_ocsp_resp()` returns the length of the OCSP response data or -1 if there is no OCSP response data.