Appendix G. Quick Reference
Prev |  |

## Appendix G. Quick Reference

    (a != b ? v1 : v2)

    #define NAME # replacement text #

    #define NAME(a' b' c') # replacement text #

    #include “filename”

    #undef NAME

              $NAME

    a %  b  (no rate restriction)

    a && b  (logical AND; not audio-rate)

    (a >  b ? v1 : v2)

    (a >= b ? v1 : v2)

    (a <  b ? v1 : v2)

    (a <= b ? v1 : v2)

    a *  b  (no rate restriction)

    + a  (no rate restriction)

    − a  (no rate restriction)

    a /  b  (no rate restriction)

    ar = xarg

    ir = iarg

    kr = karg

    (a == b ? v1 : v2)

    a ^  b  (b not audio-rate)

    a || b  (logical OR; not audio-rate)

    0dbfs = iarg

    a(x) (control-rate args only)

    abs(x) (no rate restriction)

    ir active insnum

    kr active kinsnum

    ar adsr iatt, idec, islev, irel [, idel]

    kr adsr iatt, idec, islev, irel [, idel]

    ar adsyn kamod, kfmod, ksmod, ifilcod

    ar adsynt kamp, kcps, iwfn, ifreqfn, iampfn, icnt [, iphs]

    kaft aftouch [imin] [, imax]

    ar alpass asig, krvt, ilpt [, iskip] [, insmps]

    ampdbfs(x)  (no rate restriction)

    ampdb(x)  (no rate restriction)

    iamp ampmidi iscal [, ifn]

    kr aresonk ksig, kcf, kbw [, iscl] [, iskip]

    ar areson asig, kcf, kbw [, iscl] [, iskip]

    kr atonek ksig, khp [, iskip]

    ar atone asig, khp [, iskip]

    ar atonex asig, khp [, inumlayer] [, iskip]

    a1, a2 babo asig, ksrcx, ksrcy, ksrcz, irx, iry, irz [, idiff] [, ifno]

    ar balance asig, acomp [, ihp] [, iskip]

    ar bamboo kamp, idettack [, inum] [, idamp] [, imaxshake] [, ifreq] [, ifreq1] [, ifreq2]

    a1 bbcutm asource, ibps, isubdiv, ibarlength, iphrasebars, inumrepeats [, istutterspeed] [, istutterchance] [, ienvchoice ]

    a1,a2 bbcuts asource1, asource2, ibps, isubdiv, ibarlength, iphrasebars, inumrepeats [, istutterspeed] [, istutterchance] [, ienvchoice]

    ar betarand krange, kalpha, kbeta

    ir betarand krange, kalpha, kbeta

    kr betarand krange, kalpha, kbeta

    ar bexprnd krange

    ir bexprnd krange

    kr bexprnd krange

    ar biquada asig, ab0, ab1, ab2, aa0, aa1, aa2 [, iskip]

    ar biquad asig, kb0, kb1, kb2, ka0, ka1, ka2 [, iskip]

    birnd(x) (init- or control-rate only)

    ar bqrez asig, xfco, xres [, imode]

    ar butbp asig, kfreq, kband [, iskip]

    ar butbr asig, kfreq, kband [, iskip]

    ar buthp asig, kfreq [, iskip]

    ar butlp asig, kfreq [, iskip]

    ar butterbp asig, kfreq, kband [, iskip]

    ar butterbr asig, kfreq, kband [, iskip]

    ar butterhp asig, kfreq [, iskip]

    ar butterlp asig, kfreq [, iskip]

    kr button knum

    ar buzz xamp, xcps, knh, ifn [, iphs]

    ar cabasa iamp, idettack [, inum] [, idamp] [, imaxshake]

    ar cauchy kalpha

    ir cauchy kalpha

    kr cauchy kalpha

    cent(x)

    cggoto condition, label

    ival chanctrl ichnl, ictlno [, ilow] [, ihigh]

    kval chanctrl ichnl, ictlno [, ilow] [, ihigh]

    kr checkbox knum

    cigoto condition, label

    ckgoto condition, label

    clear avar1 [, avar2] [, avar3] [...]

    ar clfilt asig, kfreq, itype, inpol [, ikind] [, ipbr] [, isba] [, iskip]

    ar clip asig, imeth, ilimit [, iarg]

    clockoff inum

    clockon inum

    cngoto condition, label

    ar comb asig, krvt, ilpt [, iskip] [, insmps]

    kr control knum

    ar1 [, ar2] [, ar3] [, ar4] convle ain, ifilcod [, ichannel]

    ar1 [, ar2] [, ar3] [, ar4] convolve ain, ifilcod [, ichannel]

    cosh(x) (no rate restriction)

    cosinv(x) (no rate restriction)

    cos(x) (no rate restriction)

    icps cps2pch ipch, iequal

    icps cpsmidib [irange]

    kcps cpsmidib [irange]

    icps cpsmidi

    cpsoct (oct)  (no rate restriction)

    cpspch (pch)  (init- or control-rate args only)

    icps cpstmid ifn

    icps cpstuni index, ifn

    kcps cpstun ktrig, kindex, kfn

    icps cpsxpch ipch, iequal, irepeat, ibase

    cpuprc insnum, ipercent

    ar cross2 ain1, ain2, isize, ioverlap, iwin, kbias

    ar crunch iamp, idettack [, inum] [, idamp] [, imaxshake]

    idest ctrl14 ichan, ictlno1, ictlno2, imin, imax [, ifn]

    kdest ctrl14 ichan, ictlno1, ictlno2, kmin, kmax [, ifn]

    idest ctrl21 ichan, ictlno1, ictlno2, ictlno3, imin, imax [, ifn]

    kdest ctrl21 ichan, ictlno1, ictlno2, ictlno3, kmin, kmax [, ifn]

    idest ctrl7 ichan, ictlno, imin, imax [, ifn]

    kdest ctrl7 ichan, ictlno, kmin, kmax [, ifn]

    ctrlinit ichnl, ictlno1, ival1 [, ictlno2] [, ival2] [, ictlno3] [, ival3] [,...ival32]

    aout cuserrnd kmin, kmax, ktableNum

    iout cuserrnd imin, imax, itableNum

    kout cuserrnd kmin, kmax, ktableNum

    ar dam asig, kthreshold, icomp1, icomp2, irtime, iftime

    dbamp(x)  (init-rate or control-rate args only)

    dbfsamp(x)  (init-rate or control-rate args only)

    db(x)

    ar dcblock ain [, igain]

    ar dconv asig, isize, ifn

    ar delay1 asig [, iskip]

    ar delayr idlt [, iskip]

    ar delay asig, idlt [, iskip]

    delayw asig

    ar deltap3 xdlt

    ar deltapi xdlt

    ar deltapn xnumsamps

    ar deltap kdlt

    aout deltapx adel, iwsize

    deltapxw ain, adel, iwsize

    ar diff asig [, iskip]

    kr diff ksig [, iskip]

    ar1 [,ar2] [, ar3] [, ar4] diskin ifilcod, kpitch [, iskiptim] [, iwraparound] [, iformat]

    dispfft xsig, iprd, iwsiz [, iwtyp] [, idbout] [, iwtflg]

    display xsig, iprd [, inprds] [, iwtflg]

    ar distort1 asig, kpregain, kpostgain, kshape1, kshape2

    ar divz xa, xb, ksubst

    ir divz ia, ib, isubst

    kr divz ka, kb, ksubst

    kr downsamp asig [, iwlen]

    ar dripwater kamp, idettack [, inum] [, idamp] [, imaxshake] [, ifreq] [, ifreq1] [, ifreq2]

    dumpk2 ksig1, ksig2, ifilname, iformat, iprd

    dumpk3 ksig1, ksig2, ksig3, ifilname, iformat, iprd

    dumpk4 ksig1, ksig2, ksig3, ksig4, ifilname, iformat, iprd

    dumpk  ksig, ifilname, iformat, iprd

    aout duserrnd ktableNum

    iout duserrnd itableNum

    kout duserrnd ktableNum

    elseif xa R xb then

              else

              endif

              endin

              endop

    ar envlpxr xamp, irise, idur, idec, ifn, iatss, iatdec [, ixmod] [,irind]

    kr envlpxr kamp, irise, idur, idec, ifn, iatss, iatdec [, ixmod] [,irind]

    ar envlpx xamp, irise, idur, idec, ifn, iatss, iatdec [, ixmod]

    kr envlpx kamp, irise, idur, idec, ifn, iatss, iatdec [, ixmod]

    event "scorechar", kinsnum, kdelay, kdur, [, kp4] [, kp5] [, ...]

    event "scorechar", "insname", kdelay, kdur, [, kp4] [, kp5] [, ...]

    ar expon ia, idur1, ib

    kr expon ia, idur1, ib

    ar exprand krange

    ir exprand krange

    kr exprand krange

    ar expsega ia, idur1, ib [, idur2] [, ic] [...]

    ar expsegr ia, idur1, ib [, idur2] [, ic] [...], irel, iz

    kr expsegr ia, idur1, ib [, idur2] [, ic] [...], irel, iz

    ar expseg ia, idur1, ib [, idur2] [, ic] [...]

    kr expseg ia, idur1, ib [, idur2] [, ic] [...]

    exp(x) (no rate restriction)

    ir filelen ifilcod

    ir filenchnls ifilcod

    ir filepeak ifilcod [, ichnl]

    ir filesr ifilcod

    ar filter2 asig, iM, iN, ib0, ib1, ..., ibM, ia1, ia2, ..., iaN

    kr filter2 ksig, iM, iN, ib0, ib1, ..., ibM, ia1, ia2, ..., iaN

    fini ifilename, iskipframes, iformat, in1 [, in2] [, in3] [, ...]

    fink ifilename, iskipframes, iformat, kin1 [, kin2] [, kin3] [,...]

    fin ifilename, iskipframes, iformat, ain1 [, ain2] [, ain3] [,...]

    ihandle fiopen ifilename, imode

    ar flanger asig, adel, kfeedback [, imaxd]

    flashtxt  iwhich, String

    ihandle FLbox "label", itype, ifont, isize, iwidth, iheight, ix, iy [, image]

    kout, ihandle FLbutBank itype, inumx, inumy, iwidth, iheight, ix, iy, iopcode [, kp1] [, kp2] [, kp3] [, kp4] [, kp5] [....] [, kpN]

    kout, ihandle FLbutton "label", ion, ioff, itype, iwidth, iheight, ix, iy, iopcode [, kp1] [, kp2] [, kp3] [, kp4] [, kp5] [....] [, kpN]

    FLcolor2 ired, igreen, iblue

    FLcolor ired, igreen, iblue

    kout, ihandle FLcount "label", imin, imax, istep1, istep2, itype, iwidth, iheight, ix, iy, iopcode [, kp1] [, kp2] [, kp3] [...] [, kpN]

    inumsnap FLgetsnap index

              FLgroupEnd

    FLgroup "label", iwidth, iheight, ix, iy [, iborder] [, image]

    FLhide ihandle

    koutx, kouty, ihandlex, ihandley FLjoy "label", iminx, imaxx, iminy, imaxy, iexpx, iexpy, idispx, idispy, iwidth, iheight, ix, iy

    kout FLkeyb kparam1 [, kparam2] ... [, kparamN]

    kout, ihandle FLknob "label", imin, imax, iexp, itype, idisp, iwidth, ix, iy [, icursorsize]

    FLlabel isize, ifont, ialign, ired, igreen, iblue

    FLloadsnap "filename"

              FLpackEnd

    FLpack iwidth, iheight, ix, iy, itype, ispace, iborder

              FLpanelEnd

    FLpanel "label", iwidth, iheight [, ix] [, iy] [, iborder]

    FLprintk2 kval, idisp

    FLprintk itime, kval, idisp

    kout, ihandle FLroller "label", imin, imax, istep, iexp, itype, idisp, iwidth, iheight, ix, iy

              FLrun

    FLsavesnap "filename"

              FLscrollEnd

    FLscroll iwidth, iheight [, ix] [, iy]

    FLsetAlign ialign, ihandle

    FLsetBox itype, ihandle

    FLsetColor2 ired, igreen, iblue, ihandle

    FLsetColor ired, igreen, iblue, ihandle

    FLsetFont ifont, ihandle

    FLsetPosition ix, iy, ihandle

    FLsetSize iwidth, iheight, ihandle

    inumsnap, inumval FLsetsnap index [, ifn]

    FLsetTextColor isize, ihandle

    FLsetText "itext", ihandle

    FLsetTextSize isize, ihandle

    FLsetTextType itype, ihandle

    FLsetVal_i kvalue, ihandle

    FLsetVal ktrig, kvalue, ihandle

    FLshow ihandle

    FLslidBnk "names", inumsliders [, ioutable] [, iwidth] [, iheight] [, ix] [, iy] [, itypetable] [, iexptable] [, istart_index] [, iminmaxtable]

    kout, ihandle FLslider "label", imin, imax, iexp, itype, idisp, iwidth, iheight, ix, iy

              FLtabsEnd

    FLtabs iwidth, iheight, ix, iy

    kout, ihandle FLtext "label", imin, imax, istep, itype, iwidth, iheight, ix, iy

              FLupdate

    ihandle FLvalue "label", iwidth, iheight, ix, iy

    ar fmb3 kamp, kfreq, kc1, kc2, kvdepth, kvrate, ifn1, ifn2, ifn3, ifn4, ivfn

    ar fmbell kamp, kfreq, kc1, kc2, kvdepth, kvrate, ifn1, ifn2, ifn3, ifn4, ivfn

    ar fmmetal kamp, kfreq, kc1, kc2, kvdepth, kvrate, ifn1, ifn2, ifn3, ifn4, ivfn

    ar fmpercfl kamp, kfreq, kc1, kc2, kvdepth, kvrate, ifn1, ifn2, ifn3, ifn4, ivfn

    ar fmrhode kamp, kfreq, kc1, kc2, kvdepth, kvrate, ifn1, ifn2, ifn3, ifn4, ivfn

    ar fmvoice kamp, kfreq, kvowel, ktilt, kvibamt, kvibrate, ifn1, ifn2, ifn3, ifn4, ivibfn

    ar fmwurlie kamp, kfreq, kc1, kc2, kvdepth, kvrate, ifn1, ifn2, ifn3, ifn4, ivfn

    ar fof2 xamp, xfund, xform, koct, kband, kris, kdur, kdec, iolaps, ifna, ifnb, itotdur, kphs, kgliss [, iskip]

    ar fof xamp, xfund, xform, koct, kband, kris, kdur, kdec, iolaps, ifna, ifnb, itotdur [, iphs] [, ifmode] [, iskip]

    ar fog xamp, xdens, xtrans, aspd, koct, kband, kris, kdur, kdec, iolaps, ifna, ifnb, itotdur [, iphs] [, itmode] [, iskip]

    ar fold asig, kincr

    ar follow2 asig, katt, krel

    ar follow asig, idt

    ar foscili xamp, kcps, xcar, xmod, kndx, ifn [, iphs]

    ar foscil xamp, kcps, xcar, xmod, kndx, ifn [, iphs]

    foutir ihandle, iformat, iflag, iout1 [, iout2, iout3,....,ioutN]

    fouti ihandle, iformat, iflag, iout1 [, iout2, iout3,....,ioutN]

    foutk ifilename, iformat, kout1 [, kout2, kout3,....,koutN]

    fout ifilename, iformat, aout1 [, aout2, aout3,...,aoutN]

    fprintks "filename", "string", [, kval1] [, kval2] [...]

    fprints "filename", "string" [, kval1] [, kval2] [...]

    frac(x) (init-rate or control-rate args only)

    ftchnls(x) (init-rate args only)

    gir ftgen ifn, itime, isize, igen, iarga [, iargb ] [...]

    ftlen(x) (init-rate args only)

    ftloadk "filename", ktrig, iflag, ifn1 [, ifn2] [...]

    ftload "filename", iflag, ifn1 [, ifn2] [...]

    ftlptim(x) (init-rate args only)

    ftmorf kftndx, iftfn, iresfn

    ftsavek "filename", ktrig, iflag, ifn1 [, ifn2] [...]

    ftsave "filename", iflag, ifn1 [, ifn2] [...]

    ftsr(x) (init-rate args only)

    ar gain asig, krms [, ihp] [, iskip]

    ar gauss krange

    ir gauss krange

    kr gauss krange

    ar gbuzz xamp, xcps, knh, klh, kmul, ifn [, iphs]

    ar gogobel kamp, kfreq, ihrd, ipos, imp, kvibf, kvamp, ivfn

    goto label

    ar grain2 kcps, kfmd, kgdur, iovrlp, kfn, iwfn [, irpow] [, iseed] [, imode]

    ar grain3 kcps, kphs, kfmd, kpmd, kgdur, kdens, imaxovr, kfn, iwfn, kfrpow, kprpow [, iseed] [, imode]

    ar grain xamp, xpitch, xdens, kampoff, kpitchoff, kgdur, igfn, iwfn, imgdur [, igrnd]

    ar granule xamp, ivoice, iratio, imode, ithd, ifn, ipshift, igskip, igskip_os, ilength, kgap, igap_os, kgsize, igsize_os, iatt, idec [, iseed] [, ipitch1] [, ipitch2] [, ipitch3] [, ipitch4] [, ifnenv]

    ar guiro kamp, idettack [, inum] [, idamp] [, imaxshake] [, ifreq] [, ifreq1]

    ar harmon asig, kestfrq, kmaxvar, kgenfreq1, kgenfreq2, imode, iminfrq, iprd

    ar1, ar2 hilbert asig

    aleft, aright hrtfer asig, kaz, kelev, “HRTFcompact”

    ar hsboscil kamp, ktone, kbrite, ibasfreq, iwfn, ioctfn [, ioctcnt] [, iphs]

    i(x) (control-rate args only)

    if ia R ib igoto label

    if ka R kb kgoto label

    if ia R ib goto label

    if xa R xb then

    igoto label

              ihold

    ar1, ar2, ar3, ar4, ar5, ar6, ar7, ar8, ar9, ar10, ar11, ar12, ar13, ar14, ar15, ar16, ar17, ar18, ar19, ar20, ar21, ar22, ar23, ar24, ar25, ar26, ar27, ar28, ar29, ar30, ar31, ar32 in32

    ar1 inch ksig1

    ar1, ar2, ar3, ar4, ar5, ar6 inh

    initc14 ichan, ictlno1, ictlno2, ivalue

    initc21 ichan, ictlno1, ictlno2, ictlno3, ivalue

    initc7 ichan, ictlno, ivalue

    ar init iarg

    ir init iarg

    kr init iarg

    ar1, ar2, ar3, ar4, ar5, ar6, ar7, ar8 ino

    ar1, ar2,  ar3, a4 inq

    ar1 in

    ar1, ar2 ins

    instr i, j, ...

    ar integ asig [, iskip]

    kr integ ksig [, iskip]

    ar interp ksig [, iskip] [, imode]

    int(x)  (init-rate or control-rate args only)

    kvalue invalue "channel name"

    ar1, ar2, ar3, ar4, ar5, ar6, ar7, ar8, ar9, ar10, ar11, ar12, ar13, ar14, ar15, ar16 inx

    inz ksig1

    kout jitter2 ktotamp, kamp1, kcps1, kamp2, kcps2, kamp3, kcps3

    kout jitter kamp, kcpsMin, kcpsMax

    ar jspline xamp, kcpsMin, kcpsMax

    kr jspline kamp, kcpsMin, kcpsMax

    kgoto label

    kr = iarg

    ksmps = iarg

    ktableseg ifn1, idur1, ifn2 [, idur2] [, ifn3] [...]

    kr lfo kamp, kcps [, itype]

    ar lfo kamp, kcps [, itype]

    ar limit asig, klow, khigh

    ir limit isig, ilow, ihigh

    kr limit ksig, klow, khigh

    ar linenr xamp, irise, idec, iatdec

    kr linenr kamp, irise, idec, iatdec

    ar linen xamp, irise, idur, idec

    kr linen kamp, irise, idur, idec

    ar line ia, idur1, ib

    kr line ia, idur1, ib

    kr lineto ksig, ktime

    ar linrand krange

    ir linrand krange

    kr linrand krange

    ar linsegr ia, idur1, ib [, idur2] [, ic] [...], irel, iz

    kr linsegr ia, idur1, ib [, idur2] [, ic] [...], irel, iz

    ar linseg ia, idur1, ib [, idur2] [, ic] [...]

    kr linseg ia, idur1, ib [, idur2] [, ic] [...]

    a1, a2 locsend

    a1, a2,  a3, a4 locsend

    a1, a2 locsig asig, kdegree, kdistance, kreverbsend

    a1, a2,  a3, a4 locsig asig, kdegree, kdistance, kreverbsend

    log10(x) (no rate restriction)

    logbtwo(x)  (init-rate or control-rate args only)

    log(x) (no rate restriction)

    ksig loopseg kfreq, ktrig, ktime0, kvalue0 [, ktime1] [, kvalue1] [, ktime2] [, kvalue2] [...]

    ax, ay, az lorenz ksv, krv, kbv, kh, ix, iy, iz, iskip

    ar [,ar2] loscil3 xamp, kcps, ifn [, ibas] [, imod1] [, ibeg1] [, iend1] [, imod2] [, ibeg2] [, iend2]

    ar [,ar2] loscil xamp, kcps, ifn [, ibas] [, imod1] [, ibeg1] [, iend1] [, imod2,] [, ibeg2] [, iend2]

    ar lowpass2 asig, kcf, kq [, iskip]

    ar lowres asig, kcutoff, kresonance [, iskip]

    ar lowresx asig, kcutoff, kresonance [, inumlayer] [, iskip]

    ar lpf18 asig, kfco, kres, kdist

    ar lpfreson asig, kfrqratio

    ar lphasor xtrns [, ilps] [, ilpe] [, imode] [, istrt] [, istor]

    lpinterp islot1, islot2, kmix

    ar lposcil3 kamp, kfreqratio, kloop, kend, ifn [, iphs]

    ar lposcil kamp, kfreqratio, kloop, kend, ifn [, iphs]

    krmsr, krmso, kerr, kcps lpread ktimpnt, ifilcod [, inpoles] [, ifrmrate]

    ar lpreson asig

    ksig lpshold kfreq, ktrig, ktime0, kvalue0  [, ktime1] [, kvalue1] [, ktime2] [, kvalue2] [...]

    lpslot islot

    ar maca asig1 [, asig2] [, asig3] [, asig4] [, asig5] [...]

    ar mac asig1, ksig1 [, asig2] [, ksig2] [, asig3] [, ksig3] [...]

    ar madsr iatt, idec, islev, irel [, idel] [, ireltim]

    kr madsr iatt, idec, islev, irel [, idel] [, ireltim]

    ar mandol kamp, kfreq, kpluck, kdetune, kgain, ksize, ifn [, iminfreq]

    ar marimba kamp, kfreq, ihrd, ipos, imp, kvibf, kvamp, ivibfn, idec [, idoubles] [, itriples]

    massign ichnl, insnum

    massign ichnl, "insname"

    maxalloc insnum, icount

    mclock ifreq

    mdelay kstatus, kchan, kd1, kd2, kdelay

    idest midic14 ictlno1, ictlno2, imin, imax [, ifn]

    kdest midic14 ictlno1, ictlno2, kmin, kmax [, ifn]

    idest midic21 ictlno1, ictlno2, ictlno3, imin, imax [, ifn]

    kdest midic21 ictlno1, ictlno2, ictlno3, kmin, kmax [, ifn]

    idest midic7 ictlno, imin, imax [, ifn]

    kdest midic7 ictlno, kmin, kmax [, ifn]

    midichannelaftertouch xchannelaftertouch [, ilow] [, ihigh]

    ichn midichn

    midicontrolchange xcontroller, xcontrollervalue [, ilow] [, ihigh]

    ival midictrl inum [, imin] [, imax]

    kval midictrl inum [, imin] [, imax]

    mididefault xdefault, xvalue

    kstatus, kchan, kdata1, kdata2 midiin

    midinoteoff xkey, xvelocity

    midinoteoncps xcps, xvelocity

    midinoteonkey xkey, xvelocity

    midinoteonoct xoct, xvelocity

    midinoteonpch xpch, xvelocity

    midion2 kchn, knum, kvel, ktrig

    midion kchn, knum, kvel

    midiout kstatus, kchan, kdata1, kdata2

    midipitchbend xpitchbend [, ilow] [, ihigh]

    midipolyaftertouch xpolyaftertouch, xcontrollervalue [, ilow] [, ihigh]

    midiprogramchange xprogram

    ar mirror asig, klow, khigh

    ir mirror isig, ilow, ihigh

    kr mirror ksig, klow, khigh

    ar moog kamp, kfreq, kfiltq, kfiltrate, kvibf, kvamp, iafn, iwfn, ivfn

    ar moogvcf asig, xfco, xres [, iscale]

    moscil kchn, knum, kvel, kdur, kpause

    ar mpulse kamp, kfreq [, ioffset]

    mrtmsg imsgtype

    ar multitap asig [, itime1] [, igain1] [, itime2] [, igain2] [...]

    mute insnum [, iswitch]

    mute "insname" [, iswitch]

    ar mxadsr iatt, idec, islev, irel [, idel] [, ireltim]

    kr mxadsr iatt, idec, islev, irel [, idel] [, ireltim]

    nchnls = iarg

    ar nestedap asig, imode, imaxdel, idel1, igain1 [, idel2] [, igain2] [, idel3] [, igain3] [, istor]

    ar nlfilt ain, ka, kb, kd, kC, kL

    ar noise xamp, kbeta

    noteoff ichn, inum, ivel

    noteondur2 ichn, inum, ivel, idur

    noteondur ichn, inum, ivel, idur

    noteon ichn, inum, ivel

    ival notnum

    ar nreverb asig, ktime, khdif [, iskip] [,inumCombs] [, ifnCombs] [, inumAlpas] [, ifnAlpas]

    nrpn kchan, kparmnum, kparmvalue

    nsamp(x) (init-rate args only)

    insno nstrnum "name"

    ar ntrpol asig1, asig2, kpoint [, imin] [, imax]

    ir ntrpol isig1, isig2, ipoint [, imin] [, imax]

    kr ntrpol ksig1, ksig2, kpoint [, imin] [, imax]

    octave(x)

    octcps (cps)  (init- or control-rate args only)

    ioct octmidib [irange]

    koct octmidib [irange]

    ioct octmidi

    octpch (pch)  (init- or control-rate args only)

    opcode name, outtypes, intypes

    ar oscbnk  kcps, kamd, kfmd, kpmd, iovrlap, iseed, kl1minf, kl1maxf, kl2minf, kl2maxf, ilfomode, keqminf, keqmaxf, keqminl, keqmaxl, keqminq, keqmaxq, ieqmode, kfn [, il1fn] [, il2fn] [, ieqffn] [, ieqlfn] [, ieqqfn] [, itabl] [, ioutfn]

    kr oscil1i idel, kamp, idur, ifn

    kr oscil1 idel, kamp, idur, ifn

    ar oscil3 xamp, xcps, ifn [, iphs]

    kr oscil3 kamp, kcps, ifn [, iphs]

    ar osciliktp kcps, kfn, kphs [, istor]

    ar oscilikt xamp, xcps, kfn [, iphs] [, istor]

    kr oscilikt kamp, kcps, kfn [, iphs] [, istor]

    ar oscilikts xamp, xcps, kfn, async, kphs [, istor]

    ar oscili xamp, xcps, ifn [, iphs]

    kr oscili kamp, kcps, ifn [, iphs]

    ar osciln kamp, ifrq, ifn, itimes

    ar oscil  xamp, xcps, ifn [, iphs]

    kr oscil  kamp, kcps, ifn [, iphs]

    ar oscils iamp, icps, iphs [, iflg]

    ar oscilx kamp, ifrq, ifn, itimes

    out32 asig1, asig2, asig3, asig4, asig5, asig6, asig7, asig8, asig10, asig11, asig12, asig13, asig14, asig15, asig16, asig17, asig18, asig19, asig20, asig21, asig22, asig23, asig24, asig25, asig26, asig27, asig28, asig29, asig30, asig31, asig32

    outch ksig1, asig1 [, ksig2] [, asig2] [...]

    outc asig1 [, asig2] [...]

    outh asig1, asig2, asig3, asig4, asig5, asig6

    outiat ichn, ivalue, imin, imax

    outic14 ichn, imsb, ilsb, ivalue, imin, imax

    outic ichn, inum, ivalue, imin, imax

    outipat ichn, inotenum, ivalue, imin, imax

    outipb ichn, ivalue, imin, imax

    outipc ichn, iprog, imin, imax

    outkat kchn, kvalue, kmin, kmax

    outkc14 kchn, kmsb, klsb, kvalue, kmin, kmax

    outkc kchn, knum, kvalue, kmin, kmax

    outkpat kchn, knotenum, kvalue, kmin, kmax

    outkpb kchn, kvalue, kmin, kmax

    outkpc kchn, kprog, kmin, kmax

    outo asig1, asig2, asig3, asig4, asig5, asig6, asig7, asig8

    outq1 asig

    outq2 asig

    outq3 asig

    outq4 asig

    outq asig1, asig2, asig3, asig4

    outs1 asig

    outs2 asig

    out asig

    outs asig1, asig2

    outvalue "channel name", kvalue

    outx asig1, asig2, asig3, asig4, asig5, asig6, asig7, asig8, asig9, asig10, asig11, asig12, asig13, asig14, asig15, asig16

    outz ksig1

    a1, a2, a3, a4 pan asig, kx, ky, ifn [, imode] [, ioffset]

    ar pareq asig, kc, kv, kq [, imode]

    ar pcauchy kalpha

    ir pcauchy kalpha

    kr pcauchy kalpha

    ibend pchbend [imin] [, imax]

    kbend pchbend [imin] [, imax]

    ipch pchmidib [irange]

    kpch pchmidib [irange]

    ipch pchmidi

    pchoct (oct)  (init- or control-rate args only)

    kr peak asig

    kr peak ksig

    pgmassign ipgm, inst

    pgmassign ipgm, "insname"

    ar phaser1 asig, kfreq, kord, kfeedback [, iskip]

    ar phaser2 asig, kfreq, kq, kord, kmode, ksep, kfeedback

    ar phasorbnk xcps, kndx, icnt [, iphs]

    kr phasorbnk kcps, kndx, icnt [, iphs]

    ar phasor xcps [, iphs]

    kr phasor kcps [, iphs]

    ar pinkish xin [, imethod] [, inumbands] [, iseed] [, iskip]

    kcps, krms pitchamdf asig, imincps, imaxcps [, icps] [, imedi] [, idowns] [, iexcps] [, irmsmedi]

    koct, kamp pitch asig, iupdte, ilo, ihi, idbthresh [, ifrqs] [, iconf] [, istrt] [, iocts] [, iq] [, inptls] [, irolloff] [, iskip]

    ax, ay, az planet kmass1, kmass2, ksep, ix, iy, iz, ivx, ivy, ivz, idelta [, ifriction]

    ar pluck kamp, kcps, icps, ifn, imeth [, iparm1] [, iparm2]

    ar poisson klambda

    ir poisson klambda

    kr poisson klambda

    ir polyaft inote [, ilow] [, ihigh]

    kr polyaft inote [, ilow] [, ihigh]

    kr portk ksig, khtim [, isig]

    kr port ksig, ihtim [, isig]

    ar poscil3 kamp, kcps, ifn [, iphs]

    kr poscil3 kamp, kcps, ifn [, iphs]

    ar poscil aamp, acps, ifn [, iphs]

    ar poscil aamp, kcps, ifn [, iphs]

    ar poscil kamp, acps, ifn [, iphs]

    ar poscil kamp, kcps, ifn [, iphs]

    ir poscil kamp, kcps, ifn [, iphs]

    kr poscil kamp, kcps, ifn [, iphs]

    powoftwo(x)  (init-rate or control-rate args only)

    ar pow aarg, kpow [, inorm]

    ir pow iarg, ipow [, inorm]

    kr pow karg, kpow [, inorm]

    prealloc insnum, icount

    prealloc "insname", icount

    printk2 kvar [, inumspaces]

    printk itime, kval [, ispace]

    printks "string", itime [, kval1] [, kval2] [...]

    print iarg [, iarg1] [, iarg2] [...]

    prints "string" [, kval1] [, kval2] [...]

    ar product asig1, asig2 [, asig3] [...]

    pset icon1 [, icon2] [...]

    p(x)

    ar pvadd ktimpnt, kfmod, ifilcod, ifn, ibins [, ibinoffset] [, ibinincr] [, iextractmode] [, ifreqlim] [, igatefn]

    pvbufread ktimpnt, ifile

    ar pvcross ktimpnt, kfmod, ifile, kampscale1, kampscale2 [, ispecwp]

    ar pvinterp ktimpnt, kfmod, ifile, kfreqscale1, kfreqscale2, kampscale1, kampscale2, kfreqinterp, kampinterp

    ar pvoc ktimpnt, kfmod, ifilcod [, ispecwp] [, iextractmode] [, ifreqlim] [, igatefn]

    kfreq, kamp pvread ktimpnt, ifile, ibin

    ar pvsadsyn fsrc, inoscs, kfmod [, ibinoffset] [, ibinincr] [, iinit]

    fsig pvsanal ain, ifftsize, ioverlap, iwinsize, iwintype [, iformat] [, iinit]

    fsig pvscross fsrc, fdest, kamp1, kamp2

    fsig pvsfread ktimpt, ifn [, ichan]

    pvsftr fsrc, ifna [, ifnf]

    kflag pvsftw fsrc, ifna [, ifnf]

    ioverlap, inumbins, iwinsize, iformat pvsinfo fsrc

    fsig pvsmaska fsrc, ifn, kdepth

    ar pvsynth fsrc, [iinit]

    ar randh xamp, xcps [, iseed] [, isize] [, ioffset]

    kr randh kamp, kcps [, iseed] [, isize] [, ioffset]

    ar randi xamp, xcps [, iseed] [, isize] [, ioffset]

    kr randi kamp, kcps [, iseed] [, isize] [, ioffset]

    ar randomh kmin, kmax, acps

    kr randomh kmin, kmax, kcps

    ar randomi kmin, kmax, acps

    kr randomi kmin, kmax, kcps

    ar random kmin, kmax

    ir random imin, imax

    kr random kmin, kmax

    ar rand xamp [, iseed] [, isel] [, ibase]

    kr rand xamp [, iseed] [, isel] [, ibase]

    ir readclock inum

    kr1, kr2 readk2 ifilname, iformat, ipol [, interp]

    kr1, kr2, kr3 readk3 ifilname, iformat, ipol [, interp]

    kr1, kr2, kr3, kr4 readk4 ifilname, iformat, ipol [, interp]

    kr readk ifilname, iformat, ipol [, interp]

    reinit label

    kflag release

    ar repluck iplk, kamp, icps, kpick, krefl, axcite

    kr resonk ksig, kcf, kbw [, iscl] [, iskip]

    ar resonr asig, kcf, kbw [, iscl] [, iskip]

    ar reson asig, kcf, kbw [, iscl] [, iskip]

    ar resonx asig, kcf, kbw [, inumlayer] [, iscl] [, iskip]

    ar resony asig, kbf, kbw, inum, ksep [, isepmode] [, iscl] [, iskip]

    ar resonz asig, kcf, kbw [, iscl] [, iskip]

    ar reverb2 asig, ktime, khdif [, iskip] [,inumCombs] [, ifnCombs] [, inumAlpas] [, ifnAlpas]

    ar reverb asig, krvt [, iskip]

    ar rezzy asig, xfco, xres [, imode]

    rigoto label

              rireturn

    kr rms asig [, ihp] [, iskip]

    ax rnd31 kscl, krpow [, iseed]

    ix rnd31 iscl, irpow [, iseed]

    kx rnd31 kscl, krpow [, iseed]

    rnd(x) (init- or control-rate only)

    ar rspline xrangeMin, xrangeMax, kcpsMin, kcpsMax

    kr rspline krangeMin, krangeMax, kcpsMin, kcpsMax

    ir rtclock

    kr rtclock

    i1,...,i16 s16b14 ichan, ictlno_msb1, ictlno_lsb1, imin1, imax1, initvalue1, ifn1,..., ictlno_msb16, ictlno_lsb16, imin16, imax16, initvalue16, ifn16

    k1,...,k16 s16b14 ichan, ictlno_msb1, ictlno_lsb1, imin1, imax1, initvalue1, ifn1,..., ictlno_msb16, ictlno_lsb16, imin16, imax16, initvalue16, ifn16

    i1,...,i32 s32b14 ichan, ictlno_msb1, ictlno_lsb1, imin1, imax1, initvalue1, ifn1,..., ictlno_msb32, ictlno_lsb32, imin32, imax32, initvalue32, ifn32

    k1,...,k32 s32b14 ichan, ictlno_msb1, ictlno_lsb1, imin1, imax1, initvalue1, ifn1,..., ictlno_msb32, ictlno_lsb32, imin32, imax32, initvalue32, ifn32

    ar samphold asig, agate [, ival] [, ivstor]

    kr samphold ksig, kgate [, ival] [, ivstor]

    ar sandpaper iamp, idettack [, inum] [, idamp] [, imaxshake]

    scanhammer isrc, idst, ipos, imult

    ar scans kamp, kfreq, ifn, id [, iorder]

    aout scantable kamp, kpch, ipos, imass, istiff, idamp, ivel

    scanu init, irate, ifnvel, ifnmass, ifnstif, ifncentr, ifndamp, kmass, kstif, kcentr, kdamp, ileft, iright, kpos, kstrngth, ain, idisp, id

    schedkwhennamed ktrigger, kmintim, kmaxnum, "name", kwhen, kdur [, ip4] [, ip5] [...]

    schedkwhen ktrigger, kmintim, kmaxnum, kinsnum, kwhen, kdur [, ip4] [, ip5] [...]

    schedkwhen ktrigger, kmintim, kmaxnum, "insname", kwhen, kdur [, ip4] [, ip5] [...]

    schedule insnum, iwhen, idur [, ip4] [, ip5] [...]

    schedule "insname", iwhen, idur [, ip4] [, ip5] [...]

    schedwhen ktrigger, kinsnum, kwhen, kdur [, ip4] [, ip5] [...]

    schedwhen ktrigger, "insname", kwhen, kdur [, ip4] [, ip5] [...]

    seed ival

    ar sekere iamp, idettack [, inum] [, idamp] [, imaxshake]

    semitone(x)

    kr sensekey

    kr sense

    ktrig_out seqtime ktime_unit, kstart, kloop, kinitndx, kfn_times

    setctrl inum, ival, itype

    setksmps iksmps

    sfilist ifilhandle

    ar sfinstr3m ivel, inotenum, xamp, xfreq, instrnum, ifilhandle [, iflag] [, ioffset]

    ar1, ar2 sfinstr3 ivel, inotenum, xamp, xfreq, instrnum, ifilhandle [, iflag] [, ioffset]

    ar sfinstrm ivel, inotenum, xamp, xfreq, instrnum, ifilhandle [, iflag] [, ioffset]

    ar1, ar2 sfinstr ivel, inotenum, xamp, xfreq, instrnum, ifilhandle [, iflag] [, ioffset]

    ir sfload "filename"

    sfpassign istartindex, ifilhandle

    ar sfplay3m ivel, inotenum, xamp, xfreq, ipreindex [, iflag] [, ioffset]

    ar1, ar2 sfplay3 ivel, inotenum, xamp, xfreq, ipreindex [, iflag] [, ioffset]

    ar sfplaym ivel, inotenum, xamp, xfreq, ipreindex [, iflag] [, ioffset]

    ar1, ar2 sfplay ivel, inotenum, xamp, xfreq, ipreindex [, iflag] [, ioffset]

    sfplist ifilhandle

    ir sfpreset iprog, ibank, ifilhandle, ipreindex

    ar shaker kamp, kfreq, kbeans, kdamp, ktimes [, idecay]

    sinh(x) (no rate restriction)

    sininv(x) (no rate restriction)

    sin(x) (no rate restriction)

    ar sleighbells kamp, idettack [, inum] [, idamp] [, imaxshake] [, ifreq] [, ifreq1] [, ifreq2]

    k1,...,k16 slider16f ichan, ictlnum1, imin1, imax1, init1, ifn1, icutoff1,..., ictlnum16, imin16, imax16, init16, ifn16, icutoff16

    i1,...,i16 slider16 ichan, ictlnum1, imin1, imax1, init1, ifn1,..., ictlnum16, imin16, imax16, init16, ifn16

    k1,...,k16 slider16 ichan, ictlnum1, imin1, imax1, init1, ifn1,..., ictlnum16, imin16, imax16, init16, ifn16

    k1,...,k32 slider32f ichan, ictlnum1, imin1, imax1, init1, ifn1, icutoff1,..., ictlnum32, imin32, imax32, init32, ifn32, icutoff32

    i1,...,i32 slider32 ichan, ictlnum1, imin1, imax1, init1, ifn1,..., ictlnum32, imin32, imax32, init32, ifn32

    k1,...,k32 slider32 ichan, ictlnum1, imin1, imax1, init1, ifn1,..., ictlnum32, imin32, imax32, init32, ifn32

    k1,...,k64 slider64f ichan, ictlnum1, imin1, imax1, init1, ifn1, icutoff1,..., ictlnum64, imin64, imax64, init64, ifn64, icutoff64

    i1,...,i64 slider64 ichan, ictlnum1, imin1, imax1, init1, ifn1,..., ictlnum64, imin64, imax64, init64, ifn64

    k1,...,k64 slider64 ichan, ictlnum1, imin1, imax1, init1, ifn1,..., ictlnum64, imin64, imax64, init64, ifn64

    k1,...,k8 slider8f ichan, ictlnum1, imin1, imax1, init1, ifn1, icutoff1,..., ictlnum8, imin8, imax8, init8, ifn8, icutoff8

    i1,...,i8 slider8 ichan, ictlnum1, imin1, imax1, init1, ifn1,..., ictlnum8, imin8, imax8, init8, ifn8

    k1,...,k8 slider8 ichan, ictlnum1, imin1, imax1, init1, ifn1,..., ictlnum8, imin8, imax8, init8, ifn8

    ar [, ac] sndwarp xamp, xtimewarp, xresample, ifn1, ibeg, iwsize, irandw, ioverlap, ifn2, itimemode

    ar1, ar2 [,ac1] [, ac2] sndwarpst xamp, xtimewarp, xresample, ifn1, ibeg, iwsize, irandw, ioverlap, ifn2, itimemode

    ar1 soundin ifilcod [, iskptim] [, iformat]

    ar1, ar2 soundin ifilcod [, iskptim] [, iformat]

    ar1, ar2, ar3 soundin ifilcod [, iskptim] [, iformat]

    ar1, ar2, ar3, ar4 soundin ifilcod [, iskptim] [, iformat]

    soundout  asig1, ifilcod [, iformat]

    a1, a2, a3, a4  space asig, ifn, ktime, kreverbsend, kx, ky

    aW, aX, aY, aZ spat3di ain, iX, iY, iZ, idist, ift, imode [, istor]

    aW, aX, aY, aZ spat3d ain, kX, kY, kZ, idist, ift, imode, imdel, iovr [, istor]

    spat3dt ioutft, iX, iY, iZ, idist, ift, imode, irlen [, iftnocl]

    k1 spdist ifn, ktime, kx, ky

    wsig specaddm wsig1, wsig2 [, imul2]

    wsig specdiff wsigin

    specdisp wsig, iprd [, iwtflg]

    wsig specfilt wsigin, ifhtim

    wsig spechist wsigin

    koct, kamp specptrk wsig, kvar, ilo, ihi, istr, idbthresh, inptls, irolloff [, iodd] [, iconfs] [, interp] [, ifprd] [, iwtflg]

    wsig specscal wsigin, ifscale, ifthresh

    ksum specsum wsig [, interp]

    wsig spectrum xsig, iprd, iocts, ifrqa [, iq] [, ihann] [, idbout] [, idsprd] [, idsinrs]

    a1, a2, a3, a4 spsend

    sqrt(x) (no rate restriction)

    sr = iarg

    ar stix iamp, idettack [, inum] [, idamp] [, imaxshake]

    ar streson asig, kfr, ifdbgain

    strset iarg, istring

    subinstrinit instrnum [, p4] [, p5] [...]

    subinstrinit "insname" [, p4] [, p5] [...]

    a1, [...] [, a8] subinstr instrnum [, p4] [, p5] [...]

    a1, [...] [, a8] subinstr "insname" [, p4] [, p5] [...]

    ar sum asig1 [, asig2] [, asig3] [...]

    alow, ahigh, aband svfilter  asig, kcf, kq [, iscl]

    ar table3 andx, ifn [, ixmode] [, ixoff] [, iwrap]

    ir table3 indx, ifn [, ixmode] [, ixoff] [, iwrap]

    kr table3 kndx, ifn [, ixmode] [, ixoff] [, iwrap]

    tablecopy kdft, ksft

    tablegpw kfn

    tableicopy idft, isft

    tableigpw ifn

    ar tableikt xndx, kfn [, ixmode] [, ixoff] [, iwrap]

    kr tableikt kndx, kfn [, ixmode] [, ixoff] [, iwrap]

    tableimix idft, idoff, ilen, is1ft, is1off, is1g, is2ft, is2off, is2g

    ar tablei andx, ifn [, ixmode] [, ixoff] [, iwrap]

    ir tablei indx, ifn [, ixmode] [, ixoff] [, iwrap]

    kr tablei kndx, ifn [, ixmode] [, ixoff] [, iwrap]

    tableiw isig, indx, ifn [, ixmode] [, ixoff] [, iwgmode]

    ar tablekt xndx, kfn [, ixmode] [, ixoff] [, iwrap]

    kr tablekt kndx, kfn [, ixmode] [, ixoff] [, iwrap]

    tablemix kdft, kdoff, klen, ks1ft, ks1off, ks1g, ks2ft, ks2off, ks2g

    ir tableng ifn

    kr tableng kfn

    ar tablera kfn, kstart, koff

    tableseg ifn1, idur1, ifn2 [, idur2] [, ifn3] [...]

    ar table andx, ifn [, ixmode] [, ixoff] [, iwrap]

    ir table indx, ifn [, ixmode] [, ixoff] [, iwrap]

    kr table kndx, ifn [, ixmode] [, ixoff] [, iwrap]

    kstart tablewa kfn, asig, koff

    tablewkt asig, andx, kfn [, ixmode] [, ixoff] [, iwgmode]

    tablewkt ksig, kndx, kfn [, ixmode] [, ixoff] [, iwgmode]

    tablew asig, andx, ifn [, ixmode] [, ixoff] [, iwgmode]

    tablew isig, indx, ifn [, ixmode] [, ixoff] [, iwgmode]

    tablew ksig, kndx, ifn [, ixmode] [, ixoff] [, iwgmode]

    ar tablexkt xndx, kfn, kwarp, iwsize [, ixmode] [, ixoff] [, iwrap]

    tablexseg ifn1, idur1, ifn2 [, idur2] [, ifn3] [...]

    ar tambourine kamp, idettack [, inum] [, idamp] [, imaxshake] [, ifreq] [, ifreq1] [, ifreq2]

    tanh(x) (no rate restriction)

    ar taninv2 ay, ax

    ir taninv2 iy, ix

    kr taninv2 ky, kx

    taninv(x) (no rate restriction)

    tan(x) (no rate restriction)

    ar tbvcf asig, xfco, xres, kdist, kasym

    ktemp tempest kin, iprd, imindur, imemdur, ihp, ithresh, ihtim, ixfdbak, istartempo, ifn [, idisprd] [, itweek]

    tempo ktempo, istartempo

    kr tempoval

    tigoto label

    kr timeinstk

    kr timeinsts

    kr timeinsts

    ir timek

    kr timek

    ir times

    kr times

    timout istrt, idur, label

    ir tival

    kr tlineto ksig, ktime, ktrig

    kr tonek ksig, khp [, iskip]

    ar tone asig, khp [, iskip]

    ar tonex  asig, khp [, inumlayer] [, iskip]

    ar transeg ia, idur, itype, ib [, idur2] [, itype] [, ic] ...

    kr transeg ia, idur, itype, ib [, idur2] [, itype] [, ic] ...

    kout trigger ksig, kthreshold, kmode

    trigseq ktrig_in, kstart, kloop, kinitndx, kfn_values, kout1 [, kout2] [...]

    ar trirand krange

    ir trirand krange

    kr trirand krange

              turnoff

    turnon insnum [, itime]

    ar unirand krange

    ir unirand krange

    kr unirand krange

    ar upsamp ksig

    aout = urd(ktableNum)

    iout = urd(itableNum)

    kout = urd(ktableNum)

    ar valpass asig, krvt, xlpt, imaxlpt [, iskip] [, insmps]

    ar1, ..., ar16 vbap16move asig, ispread, ifldnum, ifld1 [, ifld2] [...]

    ar1, ..., ar16 vbap16 asig, iazim [, ielev] [, ispread]

    ar1, ar2, ar3, ar4 vbap4move asig, ispread, ifldnum, ifld1 [, ifld2] [...]

    ar1, ar2, ar3, ar4 vbap4 asig, iazim [, ielev] [, ispread]

    ar1, ..., ar8 vbap8move asig, ispread, ifldnum, ifld1 [, ifld2] [...]

    ar1, ..., ar8 vbap8 asig, iazim [, ielev] [, ispread]

    vbaplsinit idim, ilsnum [, idir1] [, idir2] [...] [, idir32]

    vbapzmove inumchnls, istartndx, asig, idur, ispread, ifldnum, ifld1, ifld2, [...]

    vbapz inumchnls, istartndx, asig, iazim [, ielev] [, ispread]

    kfn vco2ft kcps, iwave [, inyx]

    ifn vco2ift icps, iwave [, inyx]

    ifn vco2init iwave [, ibasfn] [, ipmul] [, iminsiz] [, imaxsiz] [, isrcft]

    ar vco2 kamp, kcps [, imode] [, kpw] [, kphs] [, inyx]

    ar vcomb asig, krvt, xlpt, imaxlpt [, iskip] [, insmps]

    ar vco xamp, xcps, iwave, kpw [, ifn] [, imaxd] [, ileak] [, inyx] [, iphs]

    ar vdelay3 asig, adel, imaxdel [, iskip]

    ar vdelay asig, adel, imaxdel [, iskip]

    aout1, aout2, aout3, aout4 vdelayxq ain1, ain2, ain3, ain4, adl, imd, iws [, ist]

    aout vdelayx ain, adl, imd, iws [, ist]

    aout1, aout2 vdelayxs ain1, ain2, adl, imd, iws [, ist]

    aout1, aout2, aout3, aout4 vdelayxwq ain1, ain2, ain3, ain4, adl, imd, iws [, ist]

    aout vdelayxw ain, adl, imd, iws [, ist]

    aout1, aout2 vdelayxws ain1, ain2, adl, imd, iws [, ist]

    ival veloc [ilow] [, ihigh]

    ar vibes kamp, kfreq, ihrd, ipos, imp, kvibf, kvamp, ivibfn, idec

    kout vibrato kAverageAmp, kAverageFreq, kRandAmountAmp, kRandAmountFreq, kAmpMinRate, kAmpMaxRate, kcpsMinRate, kcpsMaxRate, ifn [, iphs]

    kout vibr kAverageAmp, kAverageFreq, ifn

    vincr asig, aincr

    ar vlowres asig, kfco, kres, iord, ksep

    ar voice kamp, kfreq, kphoneme, kform, kvibf, kvamp, ifn, ivfn

    ar vpvoc ktimpnt, kfmod, ifile [, ispecwp] [, ifn]

    ar waveset ain, krep [, ilen]

    ar weibull ksigma, ktau

    ir weibull ksigma, ktau

    kr weibull ksigma, ktau

    ar wgbowedbar kamp, kfreq, kpos, kbowpres, kgain [, iconst] [, itvel] [, ibowpos] [, ilow]

    ar wgbow kamp, kfreq, kpres, krat, kvibf, kvamp, ifn [, iminfreq]

    ar wgbrass kamp, kfreq, ktens, iatt, kvibf, kvamp, ifn [, iminfreq]

    ar wgclar kamp, kfreq, kstiff, iatt, idetk, kngain, kvibf, kvamp, ifn [, iminfreq]

    ar wgflute kamp, kfreq, kjet, iatt, idetk, kngain, kvibf, kvamp, ifn [, iminfreq] [, ijetrf] [, iendrf]

    ar wgpluck2 iplk, kamp, icps, kpick, krefl

    ar wgpluck icps, iamp, kpick, iplk, idamp, ifilt, axcite

    ar wguide1 asig, xfreq, kcutoff, kfeedback

    ar wguide2 asig, xfreq1, xfreq2, kcutoff1, kcutoff2, kfeedback1, kfeedback2

    ar wrap asig, klow, khigh

    ir wrap isig, ilow, ihigh

    kr wrap ksig, klow, khigh

    aout wterrain kamp, kpch, k_xcenter, k_ycenter, k_xradius, k_yradius, itabx, itaby

    ar xadsr iatt, idec, islev, irel [, idel]

    kr xadsr iatt, idec, islev, irel [, idel]

    xinarg1 [, xinarg2] ... [xinargN] xin

    xout xoutarg1 [, xoutarg2] ... [, xoutargN]

    kpos, kvel xscanmap iscan, kamp, kvamp [, iwhich]

    xscansmap kpos, kvel, iscan, kamp, kvamp [, iwhich]

    ar xscans kamp, kfreq, ifntraj, id [, iorder]

    xscanu init, irate, ifnvel, ifnmass, ifnstif, ifncentr, ifndamp, kmass, kstif, kcentr, kdamp, ileft, iright, kpos, kstrngth, ain, idisp, id

    xtratim iextradur

    kx, ky xyin iprd, ixmin, ixmax, iymin, iymax [, ixinit] [, iyinit]

    zacl kfirst, klast

    zakinit isizea, isizek

    ar zamod asig, kzamod

    ar zarg kndx, kgain

    ar zar kndx

    zawm asig, kndx [, imix]

    zaw asig, kndx

    ar zfilter2 asig, kdamp, kfreq, iM, iN, ib0, ib1, ..., ibM, ia1,ia2, ..., iaN

    ir zir indx

    ziwm isig, indx [, imix]

    ziw isig, indx

    zkcl kfirst, klast

    kr zkmod ksig, kzkmod

    kr zkr kndx

    zkwm ksig, kndx [, imix]

    zkw ksig, kndx

Prev | Up |
Glossary | Home |